     <ActiveSync Connection via LAN>
        0)Preparation
          -CF LAN Card compatible with NE2000
           Available CardFSOCKET LP-E (EA2906-194)APRETEC CompactLAN
          -IP address of the device

        1)Connect ActiveSync via Serial cable or USB, and make a partnership,
          then disconnect ActiveSync once.
          At this time, have Network(Ethernet)... available at the connection
          setting of ActiveSync.

	*If you write the ROM after you had made a partnership between PC and
         the device, the partnership information of PC will remain. So in this
         case, you need to make a new partnership after doing
         [delete partnership] of ActiveSync menu on PC. If you don't do this,
         the connection device will be increased like 'WinCE'A'WinCE2'... .

        *Uncheck all of checkboxes at the setting of the new partnership to
         prevent the unnecessary file synchronization and the synchronization
         error.

        2)Install LAN-ActiveSync connection tool.
          Install LAN-ActiveSync connection tool using Autorun in 
          [release\LANdebug] folder.
          <Install summary>
          -Copy ActiveSync launcher tool(ExeRepllogAs.exe) to \Nand Disk\Program
           Files.
          -Assign ActiveSync launcher tool to the right side hard icon(Setting
           hard icon) changing registry.
          -Save the registry.

        * Save the partnership setting registry of the device at the same time.
	  [HKEY_LOCAL_MACHINE\SOFTWARE\Microsoft\Windows CE Services\
	   Partners\P1]
		"PId"=dword:xxxxxxxx
		"PName"="<name of PC>"

        3)LAN connection setting
          Set the LAN connection at the Connections/New Setting.
          If you would like to use only ActiveSync, have the following setting
          default.
          -Choose 'NE2000 Compatible Ethernet Driver' from the list of LAN card
           adapter.
          -Uncheck 'Auto detect'.
          -Set IP address of the device at 'LAN IP address'.
          -Set 255.255.255.0 as Subnet mask.
          -Uncheck 'DNS Auto detect'.
          -Set IP address of PC at 'WINS1'.

	4)Insert the CF LAN Card.

        5)Tap the extreme right hard icon, then ActiveSync will start.
          If you cannot find 'Network Connection' in the list of connection,
          you need to cancel ActiveSync once and try again.
          It takes a while that the list will appear after you insert the CF
          LAN Card.

        6)Connect choosing 'Network Connection' from the list of connection.

        * If you insert the USB cable connected to PC, ActiveSync via LAN will
          be disconnected. So please don't insert the USB cable while using
          ActiveSync connection.
          But there is no problem that the USB cable has been inserted before
          you start ActiveSync connection.

        7)Disconnect ActiveSync
          Tap the extreme right hard icon, then Connection Status dialogue will
          be shown. Tap [Disconnect], then ActiveSync will be disconnected.

        *If you pull out the CF LAN Card while ActiveSync connection, PC will
         be disconnected automatically but the device will be not.
         In this case, you can disconnect ActiveSync tapping the extreme right
         hard icon. But it takes about 1 minute to end Repllog.exe, so you need
         to wait for a while to connect again.
