> 13.28 | AT^SSMSS Set Short Message Storage Sequence

> The short message storage ''MT'' (see AT+CPMS) is a logical storage. It consists of two physical storages ''ME'' and ''SM''. This command allows to select the sequence of addressing this storage.
> Syntax

> Test Command AT^SSMSS=?
> Response(s)
> ^SSMSS: (list of supported) <seq>s

> Read Command AT^SSMSS?
> Response(s)
> ^SSMSS: <seq>
> OK

> Write Command AT^SSMSS=<seq>
> Response(s)
> OK

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> SIEMENS |  | + |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <seq>(num)

> MT sequence
> 0(&F)
> ''MT'' storage is ''ME'' then ''SM
> 1
> ''MT'' storage is ''SM'' then ''ME''
> Note

> • | The <seq> parameter will be stored in non-volatile memory.