> 2.4 | Baudrate Settings on ASC0 / ASC1

> gWinSwup supports the following baudrates: 57600, 115200, 230400, 460800 Baud. The setting is relevant only for downloading the firmware over ASC0 and ASC1.
> The baudrate for the firmware download can be set regardless of the module’s baudrate configured with AT+IPR. Thus, you can take advantage of a higher baudrate (if supported by the computer’s COM port). If the baudrate selected for the download differs from the AT+IPR setting, gWinSwup briefly shows the module’s original setting before starting the download at the selected baudrate. See example in Figure 4. After successful transfer the original AT+IPR setting of the module is valid again.
> If the download aborts prematurely and, after the next attempt, completes successfully, the original baudrate cannot be restored. See issue “Download abort on ASC0 / ASC1” in Section 2.7.
> Figure 4: Different baudrate settings of module and gWinSwup
> 57600 Baud will slow down the download speed and shall be used only if the module has no valid firmware installed. See Section 2.6 and Section 2.7.