> 8.10.1 | AT^MONI responses

> ME is not connected:
> a) ME is camping on a cell and registered to the network:

> Serving Cell I Dedicated channel
> chann rs dBm MCC MNC LAC cell NCC BCC PWR RXLev C1 I chann TS timAdv PWR dBm Q ChMod
> 1013 21 -71 001 01 1001 0103 7 7 33 -105 33 I No connection

> b) ME is camping on a cell but not registered to the network (only emergency call allowed):

> Serving Cell I Dedicated channel
> chann rs dBm MCC MNC LAC cell NCC BCC PWR RXLev C1 I chann TS timAdv PWR dBm Q ChMod
> 1013 21 -71 001 01 1001 0103 7 7 33 -105 33 I Limited Service

> c) ME camping on a cell, but searching for a better cell (cell reselection):

> Serving Cell I Dedicated channel
> chann rs dBm MCC MNC LAC cell NCC BCC PWR RXLev C1 I chann TS timAdv PWR dBm Q ChMod
> 1013 21 -71 001 01 1001 0103 7 7 33 -105 33 I Cell Reselection

> d) ME is searching and could not (yet) find a suitable cell:

> Serving Cell I Dedicated channel
> chann rs dBm MCC MNC LAC cell NCC BCC PWR RXLev C1 I chann TS timAdv PWR dBm Q ChMod
> Searching

> ME is connected (Call in progress):

> Serving Cell I Dedicated channel
> chann rs dBm MCC MNC LAC cell NCC BCC PWR RXLev C1 I chann TS timAdv PWR dBm Q ChMod
> 1013 19 -76 001 01 1001 0103 7 7 33 -105 33 I 1015 1 0 5 -76 0 S_HR

> Columns for Serving Cell:

> Column | Description
> chann | ARFCN (Absolute Frequency Channel Number) of the BCCH carrier
> rs | RSSI value 0 - 63 (RSSI = Received signal strength indication)
> dBm | Receiving level of the BCCH carrier in dBm
> MCC | Mobile Country Code (first part of the PLMN code)
> MNC | Mobile Network Code (second part of the PLMN code)
> LAC | Location area code, see note
> cell | Cell ID
> NCC | PLMN colour code
> BCC | Base station colour code
> PWR | Maximal power level used on RACH channel in dBm
> RXLev | Minimal receiving level (in dBm) to allow registration
> C1 | Coefficient for base station selection

> Columns for Dedicated channel:

> Column | Description
> chann | ARFCN (Absolute Frequency Channel Number) of the TCH carrier Note: <chann> = h indicates frequency hopping.
> TS | Timeslot number
> timAdv | Timing advance in bits
> PWR | Current power level
> dBm | Receiving level of the traffic channel carrier in dBm
> Q | Receiving quality (0-7)
> ChMod | Channel mode (--: Signalling, S_HR: Half rate, S_FR: Full rate, S_EFR: Enhanced Full Rate, A_HR: AMR Half rate, A_FR: AMR Full rate)