> 22.1 | A/ Repeat previous command line

> Syntax

> Exec Command A/
> Response(s)

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> V.250 |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Command Description
> Repeat previous command line.
> Notes

> • | Line does not need to end with terminating character.

> • | After beginning with the character "a" or "A" a second character "t", "T" or "/" has to follow. In case of using a wrong second character, it is necessary to start again with character "a" or "A".

> • | If autobauding is active, the command A/ cannot be used (see AT+IPR).