> 2.16.4 | Open Internet Service

> This section comprises the subsections Description, Used AT Commands, Flow Chart and Examples. To move to these subsections please use the Navigation Frame or the appropriate buttons on the toolbar.

> 2.16.4.1 | Description

> This chapter describes how to open the service profiles configured before with the AT^SISO command. Executing that command causes bearer (GPRS/CSD) establishment.

> • | The errors, which might occur after executing the AT^SISO command in URC mode can be:

> - | Setup profile errors. They apper instead of OK answer.

> - | Bearer (GPRS/CSD) establishment errors.

> - | Service and server errors, which can appear between OK answer and the AT^SISC command.

> 2.16.4.2 | Used AT commands

> Command | Explanation
> AT^SISO | Internet Service Open

> 2.16.4.3 | Flow chart

> Figure 148: Open Internet Services

> 2.16.4.4 | Examples

> (see Write/Read chapter)