> 17.2 | AT+CNUM Read own numbers

> AT+CNUM returns the subscribers own number(s) from the SIM.
> Syntax

> Test Command AT+CNUM=?
> Response(s)
> OK

> Exec Command AT+CNUM
> Response(s)
> [+CNUM: [<alpha>], <number>, <type>]
> [+CNUM: ... ]
> OK
> ERROR
> +CME ERROR: <err>

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> GSM 07.07 |  | + |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <alpha>(str)

> Optional alphanumeric string associated with <number>.

> <number>(str)

> Phone number in format specified by <type>.

> <type>(str)

> Type of address octet, see also: AT+CPBR <type>.
> Note

> • | Users should be aware that when using this AT command quickly after SIM PIN authentication the SIM data may not yet be accessible, resulting in a short delay before the requested AT command response is returned. See Section 23.1, Restricted access to SIM data after SIM PIN authentication for further detail.