> 8.3 | AT^SOPS Extended Operator Selection

> AT^SOPS queries the present status of the TC65's network registration. Since basic operator selection services are available with AT+COPS this command uses the methods of the Enhanced Operator Name String (EONS) specification while handling operator name strings. Additional EONS related information is available with AT^SIND.
> AT^SOPS test command lists sets of five parameters, each representing an operator present in the network.
> A set consists of

> 1. | an integer indicating the availability of the operator,

> 2. | specification of the source of the operator name <eonsOperator>,

> 3. | operator name according to EONS Table,

> 4. | Service Provider Name from the SIM Service Table and

> 5. | numeric format representation of the operator.

> Any of the parameters may be unavailable and will then be an empty field (,,).
> The list of operators comes in the following order: Home network, networks referenced in SIM and other networks.
> After the operator list the TC65 returns lists of supported <mode>s and <format>s. These lists are delimited from the operator list by two commas.
> If the test command is used while an ongoing GPRS transfer, traffic will be interrupted for up to one minute.
> Command settings are effective over all serial interfaces of the TC65.
> Syntax

> Test Command AT^SOPS=?
> Response(s)
> ^SOPS:[list of present operator( <opStatus>, <eonsType>, <eonsOperator>, <servProvider>, <opName>)s ], , (list of supported <mode>)s, (list of supported <format>)s
> OK
> ERROR
> +CME ERROR: <err>

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> SIEMENS |  | + |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <opStatus>(num)

> Status
> 0
> unknown
> 1
> operator available
> 2
> current operator
> 3
> operator forbidden

> <eonsType>(num)

> Specification of the source of the operator name <eonsOperator>. Details of EONS-supplied operator name types are available at AT^SIND.

> <eonsOperator>

> Operator name; format depends on the source of the operator name, specified by <eonsType>.

> <servProvider>(str)

> Service Provider Name according to setting of Service No. 17 in the SIM Service Table (EF SST).

> <opName>

> Operator
> Operator name in numerical presentation contains the GSM Location Area Identification (LAI) number, which consists of the 3-digit Mobile Country Code (MCC) plus the 2- or 3-digit Mobile Network Code (MNC).
> Parameter is stored non-volatile to the SIM.

> <mode>(num)

> Parameter is not applicable.

> <format>(num)

> Parameter is not applicable.
> Note

> • | The AT^SOPS Test command is only accepted by the module after a valid pin has been entered.