> 21.1 | AT^SJRA Run Java Application

> The AT^SJRA write command launches the Java application.
> Syntax

> Test Command AT^SJRA=?
> Response(s)
> ("IMlet path")

> Write Command AT^SJRA=<appName>
> Response(s)
> ^SJRA:
> OK
> If not successful:
> ERROR
> +CME ERROR: <err>

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> SIEMENS |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <appName>(str)

> Path of the Java application
> The application name must be given as a fully qualified pathname (a:/.../...) to the jar/jad file containing the desired application.
> The local flash file system is identified by: A:. Directory separator is ''/'' (002Fh).
> Example: A:/java/jam/example/helloworld/helloworld.jar
> Notes

> • | As an alternative, the Java application can be enabled to start up automatically whenever TC65 is getting started. Use the AT^SCFG command to make all the settings need for the Java autostart mode.

> • | When the Java application starts, all current calls will be terminated.