> 2.11 | AT+GCAP Request complete TA capabilities list

> AT+GCAP returns a list of additional capabilities.
> Syntax

> Test Command AT+GCAP=?
> Response(s)
> OK

> Exec Command AT+GCAP
> Response(s)
> +GCAP: <name>
> OK

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> V.250 |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <name>(str)

> e.g.: +CGSM,+FCLASS
> Note

> • | +CGSM: The response text shows which GSM commands of the ETSI standard are supported.