> 15.2.2 | SAP Response Message Parameters

> The table below shows all SAP response and indication message parameters sent when

> • | an "^SRSM" URC is issued by an ME acting as SAP server

> • | and then the AT^SRSM write command is used to transfer data to the SAP client.

> SAP Response Message Parameter Mapping:

> Id | SAP Message Name | SAP parameter mapping to AT^SRSA parameters <RsaMsgId> [,<RsaMsgData> [,<RsaMsgLen> [,<RsaMsgRc>]]]
> 1 | CONNECT_RESP | 1,,<MaxMsgSize>,<ConnStatus>
> 3 | DISCONNECT_RESP | 3
> 4 | DISCONNECT_IND | 4,,,<DiscType>
> 6 | TRANSFER_APDU_RESP | 6,<RspApdu>,<RspApduLen>,<ResCode>
> 8 | TRANSFER_ATR_RESP | 8,<ATR>,<AtrLen>,<ResCode>
> 10 | POWER_SIM_OFF_RESP | 10,,,<ResCode>
> 12 | POWER_SIM_ON_RESP | 12,,,<ResCode>
> 14 | RESET_SIM_RESP | 14,,,<ResCode>
> 16 | TRANSFER_CARD_READER _STATUS_RESP | 16,,<CardRdStatus>,<ResCode>
> 17 | STATUS_IND | 17,,,<StatusChange>
> 18 | ERROR_RESP | 18
> 20 | SET_TRANSPORT_PROTOCOL_RESP | 20,,,<ResCode>