> 2.13 | AT+CSCS Select TE character set

> The AT+CSCS write command informs the TA which character set <chset> is used by the TE. This enables the TA to convert character strings correctly between TE and ME character sets. See also Section 1.5, Supported character sets.
> Note that when the TA-TE interface is set to 8-bit operation and the used TE alphabet is 7-bit, the highest bit will be set to zero.
> Syntax

> Test Command AT+CSCS=?
> Response(s)
> +CSCS: (list of supported<chset>s)
> OK

> Read Command AT+CSCS?
> Response(s)
> +CSCS: <chset>
> OK

> Write Command AT+CSCS=[<chset>]
> Response(s)
> OK

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> GSM 07.07, GSM 11.11 |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <chset>(str)

> “GSM“(&F)(P)
> GSM default alphabet (GSM 03.38 subclause 6.2.1);
> Note: This setting may cause software flow control problems since the codes used to stop and resume data flow (XOFF = decimal 19, XON = decimal 17) are interpreted as normal characters.
> “UCS2“
> 16-bit universal multiple-octet coded character set (ISO/IEC10646 [32]); UCS2 character strings are converted to hexadecimal numbers from 0000 to FFFF; e.g. "004100620063" equals three 16-bit characters with decimal values 65, 98 and 99.