> 8.1 | AT+COPN Read operator names

> The AT+COPN command returns the list of operator names from the ME. Each operator code <numericn> that has an alphanumeric equivalent <alphan> in the ME memory is returned. See also: AT^SPLM.
> Syntax

> Test Command AT+COPN=?
> Response(s)
> OK
> ERROR
> +CME ERROR

> Exec Command AT+COPN
> Response(s)
> +COPN: <numericn>, <alphan>
> +COPN: ...
> OK
> ERROR
> +CME ERROR

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> GSM 07.07 |  | + |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <numericn>(str)

> Operator in numeric format; GSM location area identification number.

> <alphan>(str)

> Operator in long alphanumeric format; can contain up to 26 characters.