> 13.18 | AT^SCML List Concatenated Short Messages from preferred store

> The write command returns messages with status value <stat> from message storage <mem1> to the TE. If the status of the message is 'received unread', the status in the storage changes to 'received read'. The execute command is the same as the write command with the given default for <stat>. See notes of AT+CMGL.
> Syntax

> Test Command AT^SCML=?
> Response(s)
> ^SCML: (list of supported <stat>s)
> OK

> Exec Command AT^SCML
> Response(s)
> ^SCML: (see write command for default of <stat>)
> OK

> Write Command AT^SCML=<stat>
> Response(s)
> Output if text mode (AT+CMGF=1) and command successful:
> For SMS-SUBMITs and/or SMS-DELIVERs
> ^SCML: <index>, <stat>, <oa>/<da>, [<alpha>], [<scts>][, <tooa>/<toda>, <length>][, <seq>, <max>, <ieia>, <ref>]
> <data>
> [... ]
> OK
> For SMS-STATUS-REPORTs
> ^SCML: <index>, <stat>, <fo>, <mr>, [<ra>], [<tora>], <scts>, <dt>, <st>
> [... ]
> OK
> For SMS-Commands
> ^SCML: <index>, <stat>, <fo>, <ct>
> [... ]
> OK
> Output if PDU mode (AT+CMGF=0) and command successful:
> For SMS- SUBMITs and/or SMS-DELIVERs
> ^SCML: <index>, <stat>, [<alpha>], <length>
> <pdu>
> [... ]
> OK
> If error is related to ME functionality
> ERROR
> +CMS ERROR

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> SIEMENS |  | + |  | + | + | + | + | + | + |  |  | - | + | -