> 10.14.8 | Configuring and Using FTP Upload (URC Mode)

> First set up a connection profile as explained in Section 10.1.1 or Section 10.1.2. Enter at least all parameters which are mandatory for the connection profile.
> Configure the service profile 1 for FTP:

> at^siss=1,srvType,ftp | Select service type FTP.
> OK
> at^siss=1,conId,0 | Select connection profile 0.
> OK
> at^siss=1,address,"ftpput://myname:mypasswd@192.168.1.2/upload/example.bin;type=i" | Specify FTP address with individual user name and password. The file "example.bin" shall be created on the FTP server.
> OK

> Make an FTP connection:

> at^siso=1 | Open the service.
> OK | Bearer is established, service is getting started.
> ^SISW: 1, 1 | FTP service is ready for upload.
> at^sisw=1,100 | Client requests to send 100 bytes.
> ^SISW: 1,100,100 | The write command response confirms that 100 bytes must be transferred now.
> 0123456789012345678901234567890123456789012345678901234567890123456789012345678901234567890123456789 | User data is transferred.
> OK
> ^SISW: 1, 1 | URC indicates that the FTP service is ready to transfer more data. Data of the last AT^SISW command is transferred to the remote host.
> at^sisw=1,0,1 | No more data available. The file "example.bin" shall be closed on the FTP server.
> OK
> ^SISW: 1, 2 | Data transfer finished successfully. The connection to the FTP server is closed.
> at^sisc=1 | Close the FTP service.