> 10.14.11 | Sending Email (Polling Mode)

> This example uses the service profile described in Section 10.14.9.

> at^siso=9 | Open the service, i.e. start to send the email.
> OK
> at^sisw=9,10 | Try to write 10 bytes.
> ^SISW: 9, 10, 0 | The service response indicates that 10 bytes can be written.
> Hallo Tom! | Write 10 bytes.
> OK
> at^sisw=9,10 | Try to write 10 bytes.
> ^SISW: 9, 0, 0 | The service response indicates that the service refuses to accept any data at the moment.
> OK
> at^sisw0=9,12 | Try to write 12 bytes.
> ^SISW: 9, 12, 0 | The service response indicates that 12 bytes can be written.
> Bye Bye Tom! | Write 12 bytes.
> OK
> at^sisw=9,0,1 | Set the <eodFlag> to mark the end of the email body.
> ^SISW: 9,0,0 | The <eodFlag> is accepted by the service.
> OK
> at^sisi=9 | Check the connection state of service profile 9.
> ^SISI: 9,5,0,22,0,0 | The command response confirms that the SMTP service is in state "5" (Closing) and that 22 bytes have been written.
> OK
> at^sisi=9 | Check the connection state of service profile 9.
> ^SISI: 9,6,0,22,0,0 | The command response confirms that the SMTP service is in state "6" (Down) and that 22 bytes have been written.
> OK
> at^sise=9 | Check error status of service profile 9.
> ^SISE: 9,0 | The command response confirms that no error occurred.
> OK
> at^sisc=9 | Close the service.
> OK