> 9.2.1 | Fasteners from German Supplier ETTINGER GmbH

> Sales contact:
> ETTINGER GmbH
> http://www.ettinger.de/main.cfm
> Phone: +49-81-046623-0
> Fax: +49-81-046623-99
> The following tables contain only article numbers and basic parameters of the listed components. For further detail and ordering information please contact Ettinger GmbH.
> Please note that some of the listed screws, spacers and nuts are delivered with the DSB75 Support Board. See comments below.

> Article number: 05.71.038 | Spacer - Aluminum / Wall thickness = 0.8mm
> Length | 3.0mm
> Material | AlMgSi-0,5
> For internal diameter | M2=2.0-2.3
> Internal diameter | d = 2.4mm
> External diameter | 4.0mm
> Vogt AG No. | x40030080.10

> Article number: 07.51.403 | Insulating Spacer for M2 Self-gripping1
> Length | 3.0mm
> Material | Polyamide 6.6
> Surface | Black
> Internal diameter | 2.2mm
> External diameter | 4.0mm
> Flammability rating | UL94-HB

> 1
> 2 spacers are delivered with DSB75 Support Board

> Article number: 05.11.209 | Threaded Stud M2.5 - M2 Type E / External thread at both ends
> Length | 3.0mm
> Material | Stainless steel X12CrMoS17
> Thread 1 / Length | M2.5 / 6.0mm
> Thread 2 / Length | M2 / 8.0mm
> Width across flats | 5
> Recess | yes
> Type | External / External

> Article number: 01.14.131 | Screw M21 DIN 84 - ISO 1207
> Length | 8.0mm
> Material | Steel 4.8
> Surface | Zinced A2K
> Thread | M2
> Head diameter | D = 3.8mm
> Head height | 1.30mm
> Type | Slotted cheese head screw

> 1
> 2 screws are delivered with DSB75 Support Board

> Article number: 01.14.141 | Screw M2 DIN 84 - ISO 1207
> Length | 10.0mm
> Material | Steel 4.8
> Surface | Zinced A2K
> Thread | M2
> Head diameter | D = 3.8mm
> Head height | 1.30mm
> Type | Slotted cheese head screw

> Article number: 02.10.011 | Hexagon Nut1 DIN 934 - ISO 4032
> Material | Steel 4.8
> Surface | Zinced A2K
> Thread | M2
> Wrench size / Ø | 4
> Thickness / L | 1.6mm
> Type | Nut DIN/UNC, DIN934

> 1
> 2 nuts are delivered with DSB75 Support Board