> 10.1.1 | Example: Default values of a CSD connection profile

> As stated earlier, the "conType" selected with AT^SICS determines all other matching profile parameters related to this "conType". Once "conType" is set in a new profile, the default values of all other related parameters are assumed. To view the default settings you can use the read command AT^SICS?.

> at^sics=1,conType,CSD | Select connection type CSD, identified by <conProfileId>1
> OK
> at^sics? | Query current profiles.
> ^SICS: 0, "conType", "" | Profile with <conProfileId> 0 is still empty.
> ^SICS: 1, "conType", "CSD" | The new CSD profile just created is indicated with all related parameters set to their default.
> ^SICS: 1, "alphabet", "0" | Character set determined with AT+CSCS applies when string parameters are input with AT^SICS.
> ^SICS: 1, "user", "" | No user name set.
> ^SICS: 1, "passwd", "*****" | Password masked with asteriks.
> ^SICS: 1, "authMode", "PAP" | Authentication protocol PAP is assumed as default.
> ^SICS: 1, "inactTO", "0" | No inactivity timeout set.
> ^SICS: 1, "calledNum", "" | No destination set.
> ^SICS: 1, "dataRate", "1" | Data rate set to 9.6 kbaud.
> ^SICS: 1, "dataType", "1" | Remote device is analog, e.g. an analog modem.
> ^SICS: 2, "conType", "" | Profile with <conProfileId> 2 is still empty.
> ^SICS: 3, "conType", "" | Profile with <conProfileId> 3 is still empty.
> ^SICS: 4, "conType", "" | Profile with <conProfileId> 4 is still empty.
> ^SICS: 5, "conType", "" | Profile with <conProfileId> 5 is still empty.
> OK