> 6.10 | AT+CIMI Request International Mobile Subscriber Identity (IMSI)

> AT+CIMI delivers the International Mobile Subscriber Identity (IMSI). The IMSI permits the TE to identify the individual SIM attached to the ME.
> Syntax

> Test Command AT+CIMI=?
> Response(s)
> OK

> Exec Command AT+CIMI
> Response(s)
> <imsi>
> OK
> ERROR
> +CME ERROR: <err>

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> GSM 07.07 |  | + |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <imsi>(str)

> International Mobile Subscriber Identity (string without quotes).