> 3.7 | AT+WS46 Select wireless network

> Syntax

> Test Command AT+WS46=?
> Response(s)
> +WS46: (list of supported<n>s)
> OK

> Read Command AT+WS46?
> Response(s)
> <n>
> OK

> Write Command AT+WS46=[<n>]
> Response(s)
> OK
> ERROR
> +CME ERROR

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> GSM 07.07 |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <n>(num)

> 12
> GSM digital cellular