> 7.15 | ATS8 Set number of seconds to wait for comma dialing modifier

> This command specifies the amount of time, in seconds, that the DCE shall pause, during signalling of call addressing information to the network (dialling), when a "," (comma) dial modifier is encountered in a dial string.
> Syntax

> Read Command ATS8?
> Response(s)
> <n>
> OK

> Write Command ATS8=<n>
> Response(s)
> OK
> ERROR

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> V.250 |  | - |  | + | - | + | + | - | - |  |  | - | + | -

> Command Description
> No effect for GSM.
> Parameter Description

> <n>(num)(&W)(&V)

> 0(&F)
> DCE does not pause when "," encountered in dial string
> 1...255
> Number of seconds to pause