> 2.20.1 | Manual restart

> This section comprises the subsections Description, Used AT Commands, Flow Chart, Hints and Example. To move to these subsections please use the Navigation Frame or the appropriate buttons on the toolbar.

> 2.20.1.1 | Description

> To reset and restart the ME use the command AT+CFUN. If configured to a fix baud rate (AT+IPR?0), the ME will send the URC “^SYSSTART” to notify that it is ready to operate. If autobauding is enabled (AT+IPR=0) there will be no notification. In this case, it is recommended to wait 3 to 5 seconds before entering the first AT command. To register to the network SIM PIN authentication is necessary after restart.

> 2.20.1.2 | Used AT commands

> Command | Explanation
> AT+CFUN | Set phone functionality

> For further details about the commands see [2].

> 2.20.1.3 | Flow chart

> Figure 178: Manual restart

> 2.20.1.4 | Hints

> Not applicable.

> 2.20.1.5 | Example

> **************************************
> Comment: Manual restart
> ***************************************
> ***************************************
> Comment: Restart and reset the ME
> ***************************************
> Subscr 1 Send: AT+CFUN=1,1
> Subscr 1 Receive: AT+CFUN=1,1
> Subscr 1 Receive: OK
> Subscr 1 Receive: ^SYSSTART