> 2.8.1 | Power Down on PC Suspend

> When the PC enters the suspend mode, the module stays in multiplexer mode. A virtual channel is activated and used to send the commands from the Registry value “PowerDown” or via the “PowerDownFrame” available from Multiplexer Protocol version 3 onwards. All pending send requests are stopped.
> When the PC wakes up the module gets an RTS impulse and the pending send buffers are re-enabled.