> 4 | Mechanical Characteristics

> Table 18: | Mechanical characteristics

> Weight | 190g
> Dimensions (max) L x W x H | 130mm x 90mm x 38mm
> Temperature range | -30°C to +65°C ambient temperature
> Protection class | IP40 (Avoid exposing TC65 Terminal to liquid or moisture, for example do not use it in a shower or bath.)
> Mechanical vibrations Amplitude | 7.5mm at 5-200Hz sinus
> Max. pulse acceleration | 30g pulse with 18 ms duration time
> Air humidity | 5...80% (non condensing)
> Class of flammability | UL94 HB
> Casing material | PC/ABS Cycoloy 1200 HF

> Figure 17: Mechanical dimensions