> 7.20 | AT+CRLP Select radio link protocol parameters for originated non-transparent data calls

> The AT+CRLP write command sets radio link protocol (RLP) parameters used when non-transparent data calls are originated. The read command returns the current settings for the supported RLP version 0.
> Syntax

> Test Command AT+CRLP=?
> Response(s)
> +CRLP: (list of supported<iws>s), (list of supported<mws>s), (list of supported<T1>s), (list of supported<N2>s)
> OK

> Read Command AT+CRLP?
> Response(s)
> +CRLP: <iws>, <mws>, <T1>, <N2>
> OK

> Write Command AT+CRLP=[<iws>[, <mws>[, <T1>[, <N2>]]]]
> Response(s)
> OK
> ERROR
> +CME ERROR: <err>

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> GSM 07.07 |  | - |  | + | - | + | + | - | - |  |  | - | + | -

> Parameter Description

> <iws>(num)(&W)(&V)

> Interworking window size (IWF to MS)
> 0...61(&F)

> <mws>(num)(&W)(&V)

> Mobile window size (MS to IWF)
> 0...61(&F)

> <T1>(num)(&W)(&V)

> Acknowledgement timer (T1 in 10 ms units)
> 39...[78](&F)...255

> <N2>(num)(&W)(&V)

> Re-transmission attempts N2
> 1...6(&F)...255