> 13.22 | AT^SLMS List SMS Memory Storage

> AT^SLMS indicates the max. capacity of each SMS storage type and the number of locations currently used.
> Syntax

> Test Command AT^SLMS=?
> Response(s)
> OK

> Exec Command AT^SLMS
> Response(s)
> ^SLMS: ''MT'',<total3>, <used3>
> ^SLMS: ''SM'',<total1>, <used1>
> ^SLMS: ''ME'',<total2>, <used2>
> OK
> ERROR
> +CMS ERROR

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> SIEMENS |  | + |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <total1>(num)

> Maximum number of messages storable in the SMS memory of the SIM (physical storage "SM")

> <total2>(num)

> Maximum number of messages storable in the SMS memory of the Mobile Equipment (physical storage "ME")

> <total3>(num)

> Sum of "SM" and "ME", indicated as "MT". Maximum number of all messages storable in the SIM memory and the Mobile Equipment memory.

> <used1>(num)

> Number of messages currently stored in the SMS memory of the SIM (physical storage "SM")

> <used2>(num)

> Number of messages currently stored in the SMS memory of the Mobile Equipment (physical storage "ME")

> <used3>(num)

> Concatenated logical SMS storages of SIM ("SM") and Mobile Equipment ("ME"). Sum of all messages currently stored, indicated as "MT".
> Note

> • | Users should be aware that when using this AT command quickly after SIM PIN authentication the SIM data may not yet be accessible, resulting in a short delay before the requested AT command response is returned. See Section 23.1, Restricted access to SIM data after SIM PIN authentication for further detail.