> 8.17 | AT^SPLR Read entry from the preferred operators list

> The AT^SPLR write command returns used entries from the SIM list of preferred operators with <indexa> between <index1> and <index2>. If <index2> is not given, only entry at <index1> is returned. The test command returns the whole index range supported by the SIM.
> See also GSM 07.07: AT+CPOL
> Syntax

> Test Command AT^SPLR=?
> Response(s)
> ^SPLR:(list of supported) <indexa>s
> OK
> ERROR
> +CME ERROR: <err>

> Write Command AT^SPLR=<index1>[, <index2>]
> Response(s)
> ^SPLR: <index1><oper>
> ^SPLR: <index2><oper>
> OK
> ERROR
> +CME ERROR: <err>

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> SIEMENS |  | + |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <index1>(num)

> Location number to start reading from

> <index2>(num)

> Location number where to stop reading

> <indexa>(num)

> Index range supported by the SIM card (between <index1> and <index2>)

> <oper>(str)

> Operator in numeric form; GSM location area identification number