> 13.9 | AT+CMSS Send short messages from storage

> The write command sends message with location value <index> from message storage <mem2> to the network (SMS-SUBMIT or SMS-COMMAND). If new recipient address <da> is given for SMS-SUBMIT, it shall be used instead of the one stored with the message. Reference value <mr> is returned to the TE on successful message delivery. Value can be used to identify message upon unsolicited delivery status report result code.
> If the optional parameter <da> is given, the old status of the short message at <index> remains unchanged (see <stat>).
> Syntax

> Test Command AT+CMSS=?
> Response(s)
> OK

> Write Command If text mode (AT+CMGF=1): AT+CMSS=<index>[, <da>[, <toda>]]
> Response(s)
> +CMSS: <mr>[, <scts>]
> OK
> If sending fails
> ERROR
> +CMS ERROR

> Write Command If PDU mode (AT+CMGF=0): AT+CMSS=<index>[, <da>[, <toda>]]
> Response(s)
> +CMSS: <mr>[, <ackpdu>]
> OK
> If sending fails
> ERROR
> +CMS ERROR

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> GSM 07.05 |  | + |  | + | + | + | + | + | + |  |  | - | - | -