> 7.8 | ATDL Redial last number used

> Syntax

> Exec Command ATDL[;]
> Response(s)
> If there is no last number or number is not valid:
> +CME ERROR
> If no dialtone (parameter ATX2 or ATX4):
> NO DIALTONE
> If busy (parameter setting ATX3 or ATX4):
> BUSY
> If connection cannot be set up:
> NO CARRIER
> If successfully connected and non-voice call (TA switches to online data mode):
> CONNECT <text>
> When TA returns to command mode after call release:
> OK
> If successfully connected and voice call:
> OK

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> V.250 |  | + |  | + | ± | + | + | ± | ± |  |  | - | - | -

> Command Description
> This command redials the last voice and data call number used in the ATD command. If terminated with semicolon ";" ATDL dials the last voice call number stored in the "LD" phonebook. Otherwise, the last dialed data or fax number will be used (not contained in the "LD" phonebook).
> Notes

> • | This command may be aborted generally by receiving a character during execution. Abortion is not possible during some states of connection setup such as handshaking.

> • | Parameter "I" and "i" only if no *#-code is within the dial string.