> 6.6 | Electromagnetic Compatibility (EMC)

> The TC65 Terminal meets EN 301489-7 requirements of equipment for vehicular and fixed use.
> Note: VPOWER voltage dip or interruption corresponding to a reduction of the supply voltage of >30% for >1ms does reset or shut down the terminal.
> The TC65 Terminal does not resist against test pulse 5 according ISO 7637-2 (load dump at ve hicles 24 volt supply voltage). The internal slow acting, not removable fuse will be damaged. It is recommended to use an external fast acting fuse I=0.8A with melting integral I 2t (0.8…1.5)A2s.
> To meet the EN55022 requirements (field strength), the SPI transfer rate has to be set =1.083Mbps, otherwise the application shall be designed to meet additional EMC measures.