> 10.6 | AT^SISC Internet Service Close

> The AT^SISC write command closes the TCP/IP connection to the remote peer which was opened with AT^SISO. All resources are released, all status information parameters, e.g. <srvState>, <unackData>, <ackData>, <rxCount> and <txCount> counters, are reset. Only the initial configuration settings are preserved. The service can be restarted any time, using the same configuration or a new one.
> Syntax

> Test Command AT^SISC=?
> Response(s)
> OK

> Write Command AT^SISC=<srvProfileId>
> Response(s)
> OK
> ERROR
> +CME ERROR: <err>

> PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> ± |  | + | + | + | + | + | + |  |  | - | - | -

> Parameter Description

> <srvProfileId>(num)

> 0...9
> <srvProfileId> specified with AT^SISS.