> 2.7 | AT\V Set CONNECT result code format

> Syntax

> Exec Command AT\V[<value>]
> Response(s)
> OK
> ERROR

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> V.250 |  | - |  | + | - | + | + | - | - |  |  | - | + | -

> Parameter Description

> <value>(num)(&W)(&V)

> [0]
> CONNECT <text> result code returned without RLP trailer
> 1(&F)
> CONNECT <text> result code returned with RLP trailer
> Notes

> • | For circuit switched data calls only.

> • | Output only if ATX parameter is set with value > 0.