> 13.4 | AT+CMGF Select SMS message format

> Syntax

> Test Command AT+CMGF=?
> Response(s)
> +CMGF: (list of supported<mode>s)
> OK

> Read Command AT+CMGF?
> Response(s)
> +CMGF: <mode>
> OK

> Write Command AT+CMGF=<mode>
> Response(s)
> OK

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> GSM 07.05 |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Command Description
> The write command specifies the input and output format of the short messages.
> Parameter Description

> <mode>(num)(&W)(&V)

> [0](&F)
> PDU mode
> 1
> Text mode