> 13.25 | AT^SMGR Read short message without setting status to REC READ

> The AT^SMGR command is a specific Siemens command which has the same syntax as AT+CMGR. The only functional difference is that the status "REC UNREAD" of a short message is not overwritten to "REC READ".
> Syntax

> Test Command AT^SMGR=?
> Response(s)
> ^SMGR:
> OK

> Write Command AT^SMGR=<index>
> Response(s)
> see AT+CMGR

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> SIEMENS |  | + |  | + | + | + | + | + | + |  |  | - | + | -

> Note

> • | Users should be aware that when using this AT command quickly after SIM PIN authentication the SIM data may not yet be accessible, resulting in a short delay before the requested AT command response is returned. See Section 23.1, Restricted access to SIM data after SIM PIN authentication for further detail.