> 4.8 | AT+ILRR Set TE-TA local rate reporting

> The command AT+ILRR controls whether or not the intermediate result code "+ILRR" is transmitted from the TA to the TE while a connection is being set up. The result code indicates the local rate. It is issued before the final result code of the connection, e.g. CONNECT, is transmitted to the TE.
> Syntax

> Test Command AT+ILRR=?
> Response(s)
> +ILRR: (list of supported <value>s)
> OK

> Read Command AT+ILRR?
> Response(s)
> +ILRR: <value>
> OK

> Write Command AT+ILRR=<value>
> Response(s)
> OK
> ERROR
> +CME ERROR

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> V.250 |  | + |  | + | - | - | + | - | - |  |  | - | + | -

> Intermediate Result Code
> +ILRR: <rate>
> Indicates local port rate setting upon connection setup.
> Parameter Description

> <value>(num)(&W)(&V)

> 0(&F)
> Disables reporting of local port rate
> 1
> Enables reporting of local port rate

> <rate>(num)

> Port rate setting upon connection setup (bps)
> 0
> Autobauding (see Section 4.9.1, Autobauding). Not supported on ASC1. Not usable with Java.
> 300
> 600
> 1200
> 2400
> 4800
> 9600
> 14400
> 19200
> 28800
> 38400
> 57600
> 115200
> 230400
> 460800