> 4.3 | Reduced Resistance between Battery and Module

> Generally, the power lines of the PCB tracks connecting the module with the battery should be as short and low resistant as possible.
> To minimize the effect of voltage drops (max. 400mV), you can decrease the GND resistance by using additional ground connections from the wireless module to the customer application. This can be done by using a screw or spring contact.