> 11.15 | AT^SGAUTH Set type of authentication for PPP connection

> Syntax

> Test Command AT^SGAUTH=?
> Response(s)
> ^SGAUTH: (list of supported <auth>s)
> OK
> ERROR
> +CME ERROR

> Read Command AT^SGAUTH?
> Response(s)
> ^SGAUTH: <auth>
> OK
> ERROR
> +CME ERROR

> Write Command AT^SGAUTH=<auth>
> Response(s)
> OK
> ERROR
> +CME ERROR

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> SIEMENS |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <auth>(num)

> Indicates types of supported authentication.
> 0
> none
> 1(&F)(P)
> PAP
> 2
> CHAP
> 3
> MS-CHAP-V1, CHAP and PAP