> 2.3 | USB Interface Connections

> The module supports a USB 2.0 Full Speed (12Mbit/s) device interface.
> For details on how to properly connect the module’s USB interface to the host application see [1]. The following table lists a selection of USB 2.0 hubs the module has been tested to operate with1:

> Table 2: | Tested USB 2.0 hubs

> Company | Product | Internet
> Hama GmbH & Co. KG | USB 2.0 Hub, 4-Way | www.hama.com
> ANUBIS Electronics Ltd. | 4-Port Mini Hub USB 2.0 | www.typhoon.de
> Belkin Corporation | Hi-Speed USB 2.0 4-Port Compact Hub | www.belkin.com
> Kensington | PocketHub USB 2.0 | www.kensington.com
> Sitecom Europe B.V. | USB 2.0 Hub | www.sitecom.com
> D-Link | 4-Port USB 2.0 Hub (DUB-H4) | www.dlink.com
> Micro-Star Int’l Co. Ltd. | Mega Hub 7-Port USB 2.0 | www.msi.com.tw
> Adaptect Inc. | AUH-4000 XHub4 | www.adaptec.com

> 1
> TC63 and XT65/XT75 do not support a generic USB 2.0 High Speed hub which translates High Speed (480 Mbit/s/) to Full Speed (12 Mbit/s). They can only be operated on a USB 2.0 root hub, i.e. a PC host working as Full Speed hub or High Speed hub in Full Speed mode. Therefore, the USB interface of a TC63 or XT65/XT75 module should be directly linked to a PC.