> 6.2 | Compliance with FCC Rules and Regulations

> As an integrated product, the TC65 Terminal is fully compliant with the grant of FCC Equipment Authorization issued for the in-built TC65 Module, and therefore, bears the label “Contains FCC ID QIPTC65”.
> The FCC Equipment Authorization Certification for the TC65 Module is listed under the
> FCC identifier QIPTC65
> IC: 267W-TC65
> granted to Siemens AG.
> The Siemens reference application of the TC65 Module registered under the above identifier is certified to be in accordance with the following Rules and Regulations of the Federal Communications Commission (FCC). Power listed is ERP for Part 22 and EIRP for Part 24.
> “This device contains GSM and GPRS Class12 functions in the 900 and 1800MHz Band which are not operational in U.S. Territories. This device is to be used only for mobile and fixed applications. The antenna(s) used for this transmitter must be installed to provide a separation distance of at least 20cm from all persons and must not be co-located or operating in conjunction with any other antenna or transmitter. Users and installers must be provided with antenna installation instructions and transmitter operating conditions for satisfying RF exposure compliance. Antennas used for this OEM module must not exceed 4.4dBi gain (GSM 1900) and 2.9dBi (GSM 850) for mobile and fixed operating configurations. This device is approved as a module to be installed in other devices.”
> Please note that changes or modifications not expressly approved by the party responsible for compliance could void the user’s authority to operate the equipment.