> 10.14.10 | Sending Email (URC Mode)

> This example uses the service profile described in Section 10.14.9.

> at^siso=9 | Open the service, i.e. start to send the email.
> OK
> ^SISW: 9, 1 | The "^SISW" URC indicates that email data can be transferred.
> at^sisw=9,87 | The email to be sent has 87 bytes.
> ^SISW: 9,87,87 | The write command response confirms that 87 bytes are available for transmission.
> Good Morning everyone, we are delighted to announce our next meeting on Sunday morning. | Write the message text.
> OK
> at^sisw=9,0,1 | Set the <eodFlag> to mark the end of the email body.
> ^SISW: 9,0,0 | The <eodFlag> is accepted by the service.
> ^SISW: 9,2 | The "^SISW" URC confirms that all data is sent successfully.
> at^sisi=9 | Check the connection state of the service profile 9.
> ^SISI: 9,6,0,87,0,0 | The command response confirms that the SMTP service is in state "6" (Down) and that 87 bytes have been transferred.
> at^sisc=9 | Close the service.
> OK