> 8.14 | AT^SHOM Display Homezone

> The AT^SHOM returns the homezone state. The result is valid only, if network registration state <stat> is 1 (registered) (see AT+CREG).
> The feature is available only for supported network operators (O2 Germany) and requires a suitable SIM card. If the homezone feature is not supported by the network operator or SIM card, result is always 0.
> Syntax

> Test Command AT^SHOM=?
> Response(s)
> OK

> Exec Command AT^SHOM
> Response(s)
> ^SHOM: <homezonestate>
> OK
> ERROR
> +CME ERROR: <err>

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> SIEMENS |  | + |  | + | + | + | + | + | + |  |  | - | - | -

> Parameter Description

> <homezonestate>(num)

> 0
> ME is out of Homezone and Cityzone
> 1
> ME is within the Homezone
> 2
> ME is within the Cityzone