> 2.5 | gWinSwup Download via USB

> • | Do not power down the ME, but close the host application or Terminal program to release the virtual COM port for the download. Ensure that there is no network activity in progress.

> • | To start the program run the gwswup_<xxyy>_<release>.exe file. Choose the virtual COM port assigned to the module’s USB interface1. Check the option “Use USB Swup”.

> • | After the download has completed close gWinSwup.

> • | Switch on the ME by using the IGT line. Then open your host application or Terminal program connected to the virtual COM port.

> Figure 5: gWinSwup download via USB

> 1
> To select a COM port number greater than given in the list you can type the number into the list box.