> 13.2 | AT+CMGC Send an SMS command

> Syntax

> Test Command AT+CMGC=?
> Response(s)
> OK

> Write Command If text mode (see AT+CMGF=1) AT+CMGC=<fo>, <ct>[, <pid>[, <mn>[, <da>[, <toda>]]]]<CR> Text can be entered <CTRL-Z>/<ESC>
> Response(s)
> +CMGC: <mr>[, <scts>]
> If sending fails
> ERROR
> +CMS ERROR

> Write Command If PDU mode (see AT+CMGF=0) AT+CMGC=<length><CR> PDU can be entered <CTRL-Z>/<ESC>
> Response(s)
> +CMGC: <mr>[, <ackpdu>]
> OK
> If sending fails
> ERROR
> +CMS ERROR

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> GSM 07.05 |  | + |  | + | + | + | + | + | + |  |  | - | - | -

> Notes

> • | After invoking the commands AT+CMGW, AT+CMGS or AT+CMGC it is necessary to wait for the prompt ">" before entering text or PDU. After the prompt a timer will be started to observe the input.

> • | At baudrates below 19200 it is recommended to use the line termination character only (refer to ATS3, default <CR>) before entering the text or PDU. Use of the line termination character followed by the response formatting character (refer to ATS4, default <LF> can cause problems