> 3.8 | Antenna Interface

> In order to send or receive data connect an external RF antenna to the SMA connector which is internally connected to the RF signal of the GSM module.
> Please consider that the recommended antenna equipment has been chosen to achieve optimum RF performance when operating the TC65 Terminal. Siemens does not accept warranty claims for damage caused by inappropriate equipment connected to the antenna connector.