> 7.4 | ATD><mem><n> Mobile originated call using specific memory and index number

> Syntax

> Exec Command ATD><mem><n>[<mgsm>];
> Response(s)
> ERROR
> +CME ERROR: <err>
> If no dialtone (parameter ATX2 or ATX4):
> NO DIALTONE
> If busy (parameter setting ATX3 or ATX4):
> BUSY
> If connection cannot be set up:
> NO CARRIER
> When TA returns to command mode after call release:
> OK
> If successfully connected:
> OK

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> V.250 |  | + |  | + | ± | + | + | ± | ± |  |  | - | - | -

> Command Description
> TA attempts to set up an outgoing call to the specified number. The termination character ";" is mandatory since dialing from a phonebook is only supported for voice calls and for sending *# codes of Supplementary Services or other functions.
> Parameter Description

> <mem>(str)

> Phonebook storage:
> For detailed description of storages see AT+CPBS.
> “FD“
> Fixed dialing phonebook
> “SM“
> SIM phonebook
> “ON“
> MSISDN list
> “ME“
> Mobile Equipment Phonebook
> “LD“
> Last number dialed phonebook
> “MC“
> Missed (unanswered received) calls list
> “RC“
> Received calls list
> “VM“
> CPHS voice mailbox phonebook

> <n>(num)

> Integer type memory location in the range of locations available in the selected memory, i.e. the index number returned by AT+CPBR.

> <mgsm>(str)

> String of GSM modifiers:
> I Activates CLIR (disables presentation of own phone number to called party)
> i Deactivates CLIR (enables presentation of own phone number to called party)
> Notes

> • | This command may be aborted generally by receiving a character during execution. Abortion is not possible during some states of connection setup such as handshaking.

> • | There is no <mem> for emergency call ("EN").

> • | The command is not applicable to data calls. Any attempt to dial a data call number from <mem> causes the result code "NO CARRIER" to appear.

> • | Parameter <mgsm> only if no *# code is within the dialing string.

> • | See ATX for setting result code and call monitoring parameters.

> • | Any string after <mgsm> and before ';' are ignored.

> Examples

> EXAMPLE 1 | To query the location number of the phonebook entry:

> AT+CPBR=1,xx

> TA returns the entries available in the active phonebook.

> EXAMPLE 2 | To dial a number from the SIM phonebook, for example the number stored to location 15:

> ATD>"SM"15;
> OK

> EXAMPLE 3 | To dial a phone number stored in the last dial memory on the SIM card:

> ATD>"LD"9;
> OK