> 5.4 | Charging

> Please refer to [1] and [2] for general information about charging. Charging can be monitored by the running Java application. The JVM is active in Charge mode and in Charge-Only mode if autostart is activated. Only a limited number of AT commands are available when the module is in Charge-Only mode. A Java application must be able to handle the Charge-Only mode and reset the module to reinstate the normal mode. See [2] for information about the Charge-Only mode. The Charge-Only mode is indicated by URC “^SYSSTART CHARGE-ONLY MODE”.
> Note: When a Java application is started in Charge-Only mode only AT Command APIs without CSD are available. The mode-indicating URC is created after issuing the very first AT command on any opened channel. To read the URC it is necessary to register a listener (see [3]) on this AT command API instance before passing the first AT command.