> 2.6 | gWinSwup Settings for Repairing Invalid Firmware

> If the ME is switched on although it has no valid software installed or is not responding, it waits 60 seconds for the download to be started. If the download does not begin, the ME switches off after the timeout.
> After starting gWinSwup check the option “No or invalid Firmware present in Module”. If the option is activated on ASC0 or ASC1, the gWinSwup program automatically reduces its baudrate to 57600 Baud. As a result, the download takes more time. If the option is checked on USB, the download takes the same time as under normal conditions.
> Do not check the option “No or invalid Firmware present in Module” if the ME is working normally. If you do so, gWinSwup will return an error message. The ME needs to be rebooted.
> See also Section 2.7 and Section 3.3.