> 11.16 | AT^SGCONF Configuration of GPRS related Parameters

> Syntax

> Test Command AT^SGCONF=?
> Response(s)
> ^SGCONF: (list of supported <llc_pdu_length_U>s), (list of supported <llc_pdu_length_I>s), (list of supported <GPRS msclass>es)
> OK

> Read Command AT^SGCONF?
> Response(s)
> ^SGCONF: <llc_pdu_length_U>, <llc_pdu_length_I>, <GPRS msclass>
> OK

> Write Command AT^SGCONF=[<llc_pdu_length_U>][, [<llc_pdu_length_I>][, [<GPRS msclass>]]]
> Response(s)
> OK
> ERROR
> +CME ERROR

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> SIEMENS |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <llc_pdu_length_U>(num)

> The maximum number of octets in an information field of Unnumbered (U) frames. Parameter is non-volatile.
> 0
> No negotiation with network (500 will be used).
> 140...500(D)...1520
> Lower values diminish performance.

> <llc_pdu_length_I>(num)

> The maximum number of octets in an information field of Combined Information (I) frames. Parameter is non-volatile.
> 0
> No negotiation with network (500 will be used).
> 140...500(D)...1520
> Lower values diminish performance.

> <GPRS msclass>(num)

> GPRS Multislot Class. The value can be one of the classes indicated with the Test command. The value set is volatile and powerup value is the maximum allowed.
> Notes

> • | +CME ERROR: invalid index: Parameter is out of range

> • | +CME ERROR: operation temporary not allowed: The command is blocked as long as GPRS is already in use (as long as mobile is GPRS attached).

> • | Writing to user profile with AT&W and restoring with AT&F are not supported.