> 20.8.1 | Using the Pulse Counter in Limit Counter Mode

> This example assumes that a 1 kHz frequency is applied at the GPIO10 pin. Limit counter mode is enabled to request the time the pulse counter needs to count a specified number of pulses.

> at^sccnt=1,1,1000 | Open pulse counter, enable Limit counter mode, request the time needed to count 1000 pulses.
> OK
> ^SCCNT: 0000001047 | "^SCCNT" URC indicates the time taken to count 1000 pulses.
> at^sccnt=1,1,2000 | Open pulse counter, enable Limit counter mode, request the time needed to count 2000 pulses.
> OK
> ^SCCNT: 0000002040 | "^SCCNT" URC indicates the time taken to count 2000 pulses.
> at^sccnt=1,1,10000 | Open pulse counter, enable Limit counter mode, request the time needed to count 10000 pulses.
> OK
> ^SCCNT: 0000010043 | "^SCCNT" URC indicates the time taken to count 10000 pulses.
> at^sccnt=1,1,20000 | Open pulse counter, enable Limit counter mode, request the time needed to count 20000 pulses.
> OK
> ^SCCNT: 0000020040 | "^SCCNT" URC indicates the time taken to count 20000 pulses.

> This example shows how to stop the Limit counter mode and close the pulse counter without waiting for the "^SCCNT" URC. Both methods have the same effect, it is up to you which one to use.

> at^sccnt=0,0 | Stop and close the pulse counter immediately, without "^SCCNT" URC being indicated.
> OK
> at^sscnt=3 | Stop and close the pulse counter immediately, without "^SCCNT" URC being indicated.
> OK