> 12.8 | AT+FTS Stop Transmission and Wait

> This command causes the TA to terminate a transmission and wait for <time> 10 millisecond intervals before sending the OK result code to the TE.
> Syntax

> Write Command AT+FTS=<time>
> Response(s)
> OK
> In on-hook mode:
> ERROR

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> TIA/EIA-578 |  | - |  | + | - | + | + | - | - |  |  | - | - | -

> Parameter Description

> <time>(num)

> no. of 10 millisecond intervals
> 0...85